For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster trim panel. Refer to Driver Knee Bolster Panel Replacement .
2. Remove the retaining screw.
3. Disconnect the electrical connector.
4. Remove the deflector from the I/P.
5. Remove the rear compartment lid switch from the deflector.

### Installation Procedure

1. Install the rear compartment lid switch to the deflector.
2. Connect the electrical connector.
3. Install the deflector to the I/P.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the retaining screw.

Tighten
Tighten the screw to 2 N·m (18 lb in)

5. Install the knee bolster trim panel. Refer to Driver Knee Bolster Panel Replacement .