For 1990-2009 cars

#### Tools Required

• | KM-900 Rear Toe Adjusting Tool

• | SA9140E Torque Angle Gage

1. Remove the rear axle control arm bolts and cage nuts. Discard the bolts and nuts.

Important: Do not tighten the bolts at this time.

2. Install new bolts leaving the inside forward bolt out.
3. Install the KM-900 into the open bolt hole.
4. Using the KM-900 , move the rear axle control arm in the direction of necessary toe correction.
5. Snug the rear axle control arm bolts.
6. Check the toe and adjust if necessary.

Notice: Refer to Fastener Notice in the Preface section.

7. Using the SA9140E , tighten the rear axle control arm bolts.

Tighten
Tighten the bolts and cage nuts to 90 N·m (66 lb ft) plus an additional 30 to 45 degrees.

8. Repeat this procedure on the opposite side.