For 1990-2009 cars

### Removal Procedure

1. Remove the wheelhouse panel-to-fascia screws.
2. Remove the rear wheelhouse panel-to-quarter panel and rocker panel cover panel push-in retainers.
3. Remove the wheelhouse panel.

Slide the top of the wheelhouse panel out of the quarter panel wheelhhouse.

### Installation Procedure

1. Position the top of the wheelhouse panel to the quarter panel.
2. Install the rear wheelhouse panel-to-quarter panel and rocker panel cover push-in retainers.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the wheelhouse panel-to-fascia screws.

Tighten
Tighten the screws to 2.8 N·m (25 lb in).