For 1990-2009 cars

### Adjustment Procedure

1. Move the control assembly into the Park position.
2. Disconnect the control cable from the transaxle range switch lever.
3. Make sure the transaxle range switch lever is in the Park position by moving the lever counterclockwise, away from the dash panel, until it clicks and can not be moved any further.
4. Release the control cable assembly adjustment lock tab at the control cable bracket on the rear powertrain mount. Use a screwdriver, awl, or pick to pry up the lock tab and lift.
5. Reconnect the control cable end to transaxle range switch lever.
6. Depress the lock tab on the control cable assembly.
7. Verify proper operation.