For 1990-2009 cars

### Removal Procedure

1. Insert a small flat-bladed tool between the top corners of the trim panel and the I/P. Pry out the trim panel.
2. Disconnect the electrical connectors.
3. Remove the heated seat switch from the bezel.

### Installation Procedure

1. Install the heated seat switch to the bezel.
2. Connect the electrical connectors to the switches.
3. Snap the trim panel into the I/P.