For 1990-2009 cars

#### Tools Required

KM-906-B Bushing Remover/Installer

### Removal Procedure

1. Remove the upper control arm. Refer to Rear Axle Upper Control Arm Replacement .
2. Using the , assemble the KM-906-70, KM-906-31, KM-906-32 and KM-906-34 and press the bushing from the control arm.
3. Remove the KM-906-70, KM-906-31, KM-906-32 and KM-906-34 and bushing.

### Installation Procedure

1. Using the , assemble the KM-906-70, KM-906-33, KM-906-35 and KM-906-34 and press the bushing into the control arm.
2. Remove the KM-906-70, KM-906-33, KM-906-35 and KM-906-34 from the control arm.
3. Install the upper control arm. Refer to Rear Axle Upper Control Arm Replacement .