For 1990-2009 cars

### Removal Procedure

1. Remove the lower dash closeout panel from the driver side.
2. Remove the lower air duct from the driver side.

Important: Removal of the accelerator pedal will provide access to the air temperature actuator.

3. Remove the accelerator pedal mounting nuts.
4. Remove the accelerator pedal.
5. Remove the lower console closeout panel.
6. Remove the air temperature actuator (1) screws.
7. Disconnect the air temperature actuator electrical connector.

### Installation Procedure

1. Connect the air temperature actuator electrical connector.
2. Install the air temperature actuator (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the air temperature actuator screws.

Tighten
Tighten the screws to 1 N·m (9 lb in).

4. Install the lower console closeout panel.
5. Install the accelerator pedal to the cowl.
6. Install the accelerator pedal mounting nuts.

Tighten
Tighten the nuts to 10 N·m (89 lb in).

7. Install the lower air duct.
8. Install the lower dash closeout panel.