For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the steering gear heat shield to frame bolts.
3. Remove the heat shield from the vehicle.

### Installation Procedure

1. Position the heat shield to the frame.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the steering gear heat shield to frame bolts.

Tighten
Tighten the bolts to 4 N·m (35 lb in).

3. Lower the vehicle.