For 1990-2009 cars

### Terminal Removal Procedure

If the terminal is visibly damaged or is suspected of having a faulty connection, the terminal should be replaced.

Follow the steps below in order to repair pull-to-seat connectors.

1. Remove the connector position assurance (CPA) device and/or the secondary lock.
2. Disconnect the connector from the component or separate the connectors for in-line connectors.
3. Remove the terminal position assurance (TPA) device.
4. Insert the proper pick or removal tool into the front of the connector body.

### Terminal Repair Procedure

Pull-to-seat connector repair kits are available through Saturn Service Parts. The repair kits include the connector with terminals attached to a short length of the wire and splice sleeves. Use these kits if the pull-to-seat connectors need to be repaired.