For 1990-2009 cars

### Luggage Compartment

The rear compartment release circuit consists of the following:

• | The intergrated body control module (IBCM) fuse

• | The rear compartment lid release relay

• | The rear compartment lid lock release actuator

• | The rear compartment lid release switch

• | The cargo lamp/trunk ajar switch

The rear compartment release circuit operates as follows. Battery positive voltage is applied at all times to the rear compartment lid release relay. The rear compartment lid release relay is energized by either depressing the rear compartment lid release switch, or when the IBCM receives a rear compartment release signal from a key fob. The IBCM then provides a path to ground on the rear compartment lid release relay control circuit, energizing the rear compartment lid release relay. When the rear compartment lid release relay is energized, battery positive voltage is supplied to the rear compartment lid lock release actuator causing the actuator to energize releasing the rear compartment lid. The rear compartment may be released with the dash mounted rear compartment release switch. The ignition must be in the OFF or ACCESSORY positions for the rear compartment to be released with a keyless entry transmitter fob (RFA). The rear compartment may also be released by an OnStar commanded using RFA functionality.