For 1990-2009 cars

### Removal Procedure

1. Open and support the hood.
2. Remove the push-in retainers from the hood insulator.
3. Remove the hood insulator from the hood.

### Installation Procedure

1. Position the rear edge of the hood insulator to the retainer tabs.
2. Install the 2 center push-in retainers.
3. Align the insulator as necessary and Install the remainder of the push-in retainers.
4. Close the hood.