For 1990-2009 cars

### Installation Procedure

1. Assemble the camshaft cover and gasket. Ensure that the gasket is located in the retaining groove on the camshaft cover.
2. Install the cover on the cylinder head and hand tighten the bolts.
3. Install the front lift bracket and tighten the bolts.

Tighten
Tighten the front lift bracket bolts to 25 N·m (18 lb ft).

4. Install the rear lift bracket and tighten the bolts.

Tighten
Tighten the rear lift bracket bolts to 25 N·m (18 lb ft).

5. Install the ground strap.

Tighten

• | Tighten the camshaft cover bolts to 10 N·m (89 lb in).

• | Tighten the camshaft cover ground strap bolts to 10 N·m (89 lb in).

6. Install the spark plugs.
7. Install the ignition coil and module assembly to the cam cover.

Tighten
Tighten the ignition coil-to-camshaft cover bolts to 8 N·m (71 lb in).

8. Install the power steering pump, if equipped.

Tighten
Tighten the power steering pump to 25 N·m (18 lb ft).