For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Cover and Pad Replacement .
2. Remove the right and the left carpet retainers. Refer to Carpet Retainer Replacement .
3. Remove front seat bolts.
4. Remove the center console extensions by pulling gently at the fastener location.
5. Remove the center console fasteners.
6. Tilt the front seats and console upward to allow carpet to be removed from under seat and console.
7. Remove the carpet from the vehicle.

### Installation Procedure

1. Install the rear carpet in the vehicle making sure that the carpet is properly fit under the front seat and console.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front seat bolts.

Tighten
Tighten the bolts to 25 N·m (19 lb ft).

3. Install the console fasteners.

Tighten
Tighten the fasteners to 2.5 N·m (22 lb in).

4. Install the console extensions.
5. Install the right and the left carpet retainers. Refer to Carpet Retainer Replacement .
6. Install the rear seat cushion. Refer to Rear Seat Cushion Cover and Pad Replacement .