For 1990-2009 cars

#### Fluid Capacities

Application | Specification
--- | ---
Metric | English
Important: All capacities are approximate. When adding, be sure to fill to the appropriate level as recommended in this manual.
Air Conditioning Refrigerant R134a | 0.95 kg | 2.1 lbs
Cooling System

• | 2.2L, (RPO L61) MFI, DOHC Engine

• | 3.0L, (RPO L81) MFI, DOHC Engine

• | 7.0 liters

• | 8.0 liters

• | 7.4 quarts

• | 8.5 quarts

Engine Oil with Filter

• | 2.2L, (RPO L61) MFI, DOHC Engine

• | 3.0L, (RPO L81) MFI, DOHC Engine

• | 4.7 liters

• | 4.7 liters

• | 5.0 quarts

• | 5.0 quarts

Fuel Tank | 59.4 liters | 15.7 gallon
Automatic Transaxle | 6.5 liters | 6.9 quarts
Wheel Nut Torque | 125 N·m | 92 lb ft
Engine Specifications

• | 2.2L, (RPO L61) (VIN F) MFI, DOHC Engine

• | 3.0L, (RPO L81) (VIN R) MFI, DOHC Engine

• | Automatic

• | Automatic

• | 1.14 mm (0.045 in)

• | 1.02 mm (0.040 in)