For 1990-2009 cars

## Relay Replacement Within an Electrical Center

### Removal Procedure

1. Remove the electrical center cover.
2. Locate the relay. Refer to Electrical Center Identification Views to locate the electrical center where the relay exists.

Important:

• | Always note the orientation of the relay.

• | Ensure that the electrical center is secure, as not to put added stress on the wires or terminals.

3. Remove the relay from the electrical center.

### Installation Procedure

1. Install the relay in the same position as removed.
2. Install the electrical center cover.