For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Cable Terminals | 17 N·m | 13 lb ft
Battery Feed Cable-to-UHFB | 16 N·m | 12 lb ft
Battery Hold Down Bracket Fasteners | 20 N·m | 15 lb ft
Battery Tray Fasteners | 15 N·m | 11 lb ft
Clutch Master Cylinder Mounting Nuts | 20 N·m | 15 lb ft
Clutch Pedal Asm-to-Front of Dash Nuts | 20 N·m | 15 lb ft
Clutch Pedal Bracket-to-I/P Beam Fasteners | 20 N·m | 15 lb ft
Flywheel-to-Crankshaft Bolts | 53 N·m + 25° | 39 lb ft + 25°
Pressure Plate-to-Flywheel Bolts | 15 N·m | 11 lb ft
Radio Amplifier Retaining Fasteners | 10 N·m | 89 lb in
Slave Cylinder Fasteners | 10 N·m | 89 lb in
UHFB Case Bolt | 9 N·m | 89 lb in