For 1990-2009 cars

### Removal Procedure

1. Remove the front door inner trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the inside door weatherstrip.
4. Remove the outside rear view mirror. Refer to Power Mirror Replacement or Manual Mirror Replacement .
5. Remove the outer front door panel. Refer to Front Side Door Outer Panel Replacement .
6. Remove the front door sound insulator. Refer to Front Side Door Insulator Replacement .
7. Remove the front door window run channel. Refer to Front Side Door Window Channel Replacement .
8. Remove the front door window. Refer to Front Side Door Window Replacement .
9. Remove the front door rear applique. Refer to Front Door Frame Applique Replacement .
10. Remove the outside front window run channel weatherstrip.

### Installation Procedure

1. Install the outside front window run channel weatherstrip.
2. Install the front door rear applique. Refer to Front Door Frame Applique Replacement .
3. Install the front door window. Refer to Front Side Door Window Replacement .
4. Install the front door window run channel. Refer to Front Side Door Window Channel Replacement .
5. Install the inside door weatherstrip.
6. Inspect the front door window operation.
7. Adjust the front door window , if required. Refer to Front Side Door Window Adjustment .
8. Install the outer front door panel. Refer to Front Side Door Outer Panel Replacement .
9. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
10. Install the outside rear view mirror. Refer to Power Mirror Replacement or Manual Mirror Replacement .
11. Install the front door inner trim panel. Refer to Front Side Door Trim Panel Replacement .