For 1990-2009 cars

### Removal Procedure

1. Remove the engine mount. Refer to Engine Mount Replacement .
2. Remove the engine mount bracket to engine bolts.
3. Remove the engine mount bracket from the engine.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the engine mount bracket to the engine.

Tighten
Tighten the engine mount bracket to engine bolts to 90 N·m (66 lb ft).

2. Install the engine mount. Refer to Engine Mount Replacement .