For 1990-2009 cars

### Removal Procedure

1. Pull on the lower part of the knee bolster trim panel rearwards in vehicle in order to disengage the retaining clips.
2. Repeat step 1 for the top part of the trim panel.
3. Remove the trim panel from the instrument panel (I/P).

### Installation Procedure

1. Line up the clips on the trim panel to the I/P.
2. Starting from the top of the trim panel, push the trim panel until the clips are fully seated.