For 1990-2009 cars

### Removal Procedure

1. Remove the cover/pad from the front seat back cushion. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .

Important: A heat gun may be required to aid in loosening the heat pad from the foam.

2. After removing the seat back cover, gently peel the heat pad from the seat foam.

### Installation Procedure

1. Peel off the self-stick paper from the heat pad.
2. Position the heat pad on the foam and gently press to adhere the heat pad to the foam.
3. Install the cover/pad to the seat back cushion . Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .