For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Frame to Body Bolts

- First Pass

90 N·m

66 lb ft

- Second Pass

+45-90°

Inner Tie Rod | 95 N·m | 70 lb ft
Intermediate Steering Shaft Pinch Bolt | 30 N·m | 22 lb ft
Outer Tie Rod Torque Prevailing Nut | 60 N·m | 44 lb ft
Oxygen Sensor Clamp to Underbody Nut | 4 N·m | 35 lb in
Power Steering Hose Clamps | 2.5 N·m | 22 lb in
Power Steering Hose to Cylinder Head Bolt | 10 N·m | 89 lb in
Power Steering Hose/Pipe Fitting | 27 N·m | 20 lb ft
Power Steering Hose to Transaxle Bolt | 10 N·m | 89 lb in
Power Steering Pump to Bracket Bolts | 20 N·m | 15 lb ft
Power Steering Pump to Cylinder Head Bolts | 25 N·m | 18 lb ft
Power Steering Pump Pulley bolts | 20 N·m | 15 lb ft
Remote Reservoir to Radiator Support Bolts | 7 N·m | 62 lb in
Steering Gear to Frame Bolts

- First Pass

45 N·m

35 lb ft

- Second Pass

+90-105°

Steering Gear Shield Bolts | 4 N·m | 35 lb in
Suspension Support Bolts

- First Pass

90 N·m

66 lb ft

- Second Pass

+45-90°

Transmission Mount to Frame Bolt | 26 N·m | 44 lb ft
Transmission Mount to Frame Bolt, Rear | 60 N·m | 44 lb ft
Transmission Mount Through Bolt | 90 N·m | 66 lb ft