For 1990-2009 cars

### Removal Procedure

1. Remove the front seat assembly. Refer to Front Seat Replacement - Bucket .
2. Remove the front seat back cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
3. Pull on the lumbar knob spacer to remove.
4. Remove the lumbar actuator cable screws from the seat frame.
5. Remove wire retainers from the lumbar assembly. Remove the lumbar assembly from the frame.

### Installation Procedure

1. Install the lumbar assembly to the frame. Snap the wire retainers into place.
2. Route the lumbar actuator cable and the actuator to the seat back frame.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the lumbar actuator with the fasteners.

Tighten
Tighten the fasteners to 3 N·m (27 lb in).

4. Install the lumbar knob spacer.
5. Install the seat back cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement .
6. Install the front seat assembly. Refer to Front Seat Replacement - Bucket .