For 1990-2009 cars

### Removal Procedure

1. Remove the left lower I/P closeout panel (hush panel) push pins.
2. Remove the left lower I/P closeout panel (hush panel) from the vehicle.
3. Remove the HVAC duct push pin and remove the duct from the vehicle.
4. Remove the wire harness channel from the clutch pedal bracket.
5. Disconnect the clutch start switch electrical connector.
6. Remove the clutch start switch.
7. Insert the feeler gage between the switch and clutch pedal bracket to release the switch locking tab.
8. Slide the switch downward to remove from bracket.
9. Disconnect the clutch cruise switch electrical connector.
10. Remove the clutch cruise switch.

10.1. | Slide out the red locking collar.

10.2. | Depress the side tabs and remove the switch.

### Installation Procedure

1. Install the clutch start switch.
2. Insert the tabs of the switch in the bracket and slide the switch upward until the locking tab engages.
3. Install the clutch cruise switch.

3.1. | Pull out the red locking collar.

3.2. | Depress the sides and install the switch.

3.3. | Slide the red locking collar back into the lock position.

4. Connect the clutch cruise switch and clutch start switch electrical connectors.
5. Install the clutch master cylinder push rod to clutch pedal.
6. Install the wire harness channel.
7. Install the HVAC duct work.
8. Install the left lower I/P closeout panel (hush panel).