For 1990-2009 cars

# HVAC

## All Component Locator

- HVAC Component Views

## All Description and Operation

- Air Delivery Description and Operation
- Air Temperature Description and Operation

## All Special Tools and Equipment

- Special Tools

## All Visual Identification

- HVAC Connector End Views

## Diagnostic Procedures

- Air Delivery Improper
- Air Recirculation Malfunction
- Blower Motor Always On
- Blower Motor Inoperative
- Blower Motor Malfunction
- Diagnostic System Check - HVAC Systems - Automatic
- HVAC Compressor Clutch Does Not Disengage
- HVAC Compressor Clutch Does Not Engage
- Symptoms - HVAC Systems - Automatic
- Too Cold in Vehicle
- Too Hot in Vehicle

## Diagnostic Trouble Codes

- Diagnostic Trouble Code (DTC) List
- DTC B0130
- DTC B0160, B0161, B0165, or B0166
- DTC B0185 or B0186
- DTC B0413
- DTC P0530, P0532, or P0533
- DTC P0645, P0646, or P0647

## Electrical/Electronic Schematic Diagrams

- HVAC Schematics

## General Diagnostic Information

- Scan Tool Data Definitions
- Scan Tool Data List
- Scan Tool Output Controls

## Mechanical Specifications

- Fastener Tightening Specifications

## Removal, Installation, and Replacement

- Air Inlet Valve Actuator Replacement
- Ambient Air Temperature Sensor Replacement
- Blower Motor Control Processor Replacement
- HVAC Control Module Replacement
- Inside Air Temperature Sensor Aspirator Replacement
- Mode Control Cam Replacement
- Mode Valve Actuator Replacement
- Temperature Valve Actuator Replacement