For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Raise the window in the full up position.
4. Remove the front door inside handle. Refer to Front Side Door Inside Handle Replacement .
5. Remove the bolt from the run channel.
6. Remove the weatherstrip and window run channel from the front door.

### Installation Procedure

1. Install the window run channel and weatherstrip by sliding up into the hook latch slot.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolt to the window run channel.

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Install the front door inside handle. Refer to Front Side Door Inside Handle Replacement .
4. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
5. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .