For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and the wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the brake caliper. Refer to Front Brake Caliper Replacement .
4. Remove front brake caliper bracket bolts (1).
5. Remove the front brake caliper bracket from the steering knuckle.

### Installation Procedure

1. Install the caliper bracket to the steering knuckle.
2. Coat the caliper bracket bolts (1) with 272 Threadlocker, GM P/N 12345493 or equivalent.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the new caliper bracket bolts (1).

Tighten
Tighten the caliper bracket bolts (1) to 95 N·m (70 lb ft).

4. Install the brake caliper. Refer to Front Brake Caliper Replacement .
5. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
6. Lower the vehicle.