For 1990-2009 cars

#### Tools Required

J 43653 Flywheel Holding Tool

Notice: Ensure that the correct bolts are used when installing manual transaxle flywheel or automatic transaxle flexplate. If the incorrect bolts are used, powertrain damage may result.

1. Install the flywheel.
2. Install the new bolts.

Notice: Refer to Fastener Notice in the Preface section.

3. Holding the flywheel with the J 43653 , tighten the bolts evenly.

Tighten
Tighten the flywheel bolt to 53 N·m (39 lb ft) plus 25 degrees.