For 1990-2009 cars

### Removal Procedure

1. Tape the roof panel in front of the sunroof opening using masking tape
2. Cycle the sunroof window to the vent position.
3. Slide the sunshade rearward.
4. Remove the sunroof window screws (1) on both sides.
5. Lift the sunroof window (3) up from the sunroof opening.

### Installation Procedure

1. Position the sunroof window (3) into the sunroof opening.

Ensure that the window trade mark points rearward.

2. Install the sunroof window screws (1). Do not tighten the screws.
3. Carefully close the sunroof window from the vent position to the full closed position.
4. Adjust the sunroof window. Refer to Sunroof Window Height and Opening Fit Adjustment .