For 1990-2009 cars

### Removal Procedure

1. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement .
2. Press the tabs while pulling the switch assembly outwards.
3. Disconnect the wire connector.
4. Remove the switch.

### Installation Procedure

1. Install the wire connector.
2. Slide the switch assembly until it clicks in place.
3. Install the steering column trim covers. Refer to Steering Column Trim Covers Replacement .