For 1990-2009 cars

1. Open the hood. See Hood Release for more information.
2. Remove push-pin fasteners from the grill assembly.
3. Tilt the grill assembly forward and lift it up to remove it from the vehicle.
4. Remove the fasteners from the headlamp assembly.
5. Push the headlamp housing lever up to disengage the headlamp housing from the headlamp housing pocket.
6. Rotate the bulb socket being replaced counterclockwise 1/4 of a turn while pressing the socket in firmly. Pull the socket rearward until the bulb clears the headlamp housing, and lift it up to access the bulb.
7. Disconnect the wire connector from the bulb by lifting the lock tab and pulling it away from the plastic base.
8. Remove the bulb assembly and replace it with the appropriate bulb.