For 1990-2009 cars

### Removal Procedure

1. Remove the lower I/P hush panel.
2. Disconnect the accelerator cable from the pedal by sliding the cable upward.
3. Remove the accelerator pedal to bulkhead fasteners.
4. Remove the accelerator pedal from the vehicle.

### Installation Procedure

1. Install the accelerator pedal into the vehicle and tighten the fasteners.

Tighten
Tighten the accelerator pedal-to-front of dash to 10 N·m (89 lb in).

2. Install the accelerator pedal cable.
3. Install the lower I/P hush panel.