For 1990-2009 cars

#### Tools Required

• | J 23907 Slide Hammer with Bearing Adaptor

• | J 36511 Oil Plug Hex Bit

• | J 36800 Shift Rail Bushing Remover

Important: Only remove the shift rail bearings if faulty.

1. Use the J 23907 (1) and J 36800 (2) in order to remove the front shift rail bearing from the clutch housing.
2. Use the J 36511 in order to remove the oil fill plug.
3. Remove the vent if necessary. The vent is pressed into the case and can be removed with a pair of pliers.
4. Inspect the input shaft bearing. Refer to Bearings and Spacers Cleaning and Inspection .
5. Remove the input shaft bearing if faulty.
6. Inspect the front countershaft bearing race. Refer to Bearings and Spacers Cleaning and Inspection .
7. Remove the front countershaft race if faulty.

• | Use a punch to bend in one side of the race.

• | Work the race out of the case.