For 1990-2009 cars

### Fog Lamp Bulb Replacement

1. Reach up from underneath the front body panel, rotate the bulb socket counter-clockwise 1/4 of a turn while pressing the socket in firmly. Pull the socket rearward until the bulb clears the fog lamp housing.
2. Disconnect the wire connector from the bulb by lifting the lock tab and pulling it away from the plastic base.
3. Remove the bulb assembly and replace it with the appropriate bulb.