For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Headlights/Daytime Running Lights (DRL) Schematics
1 | Did you perform the Lighting System Diagnostic System Check? | Go to Step 2 | Go to Diagnostic System Check - Lighting Systems
2 |

1. Turn ON the ignition, with the engine OFF.
2. Observe the high beam indicator on the instrument cluster.

Does the indicator illuminate during the bulb check?

Go to Step 3

Go to Step 4

3 |

1. Place the headlamp switch in the HEADLAMP position.
2. Place the headlamp dimmer switch in the HIGH position.

Does the indicator illuminate?

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

Go to Step 5

4 | Inspect for poor connections at the harness connector of the instrument panel cluster (IPC). Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 8 | Go to Step 6
5 | Inspect for poor connections at the harness connector of the body control module (BCM). Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 8 | Go to Step 7
6 | Replace the IPC. Refer to Instrument Cluster Replacement in Instrument Panel, Gages and Console. Did you complete the replacement? | Go to Step 8 | --
7 | Important: Perform the set up procedure for the BCM. Replace the BCM. Refer to Body Control Module Replacement in Body Control Systems. Did you complete the replacement? | Go to Step 8 | --
8 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2