For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor Front Bracket-to-Block | 54 N·m | 40 lb ft
A/C Compressor Front/Rear Bracket-to-Block/Head | 30 N·m | 22 lb ft
A/C Compressor-to-Front Bracket | 49 N·m | 36 lb ft
A/C Compressor-to-Rear Bracket | 25 N·m | 19 lb ft
Accelerator Bracket Assembly-to-Front of Dash | 12 N·m | 106 lb in
Accelerator Control Cable Bracket-to-Intake Manifold (L24/LL0) | 30 N·m | 22 lb ft
Air Cleaner/Resonator Attachment Bolts (All) | 10 N·m | 89 lb in
Axle Shaft Intermediate Bracket-to-Block | 55 N·m | 41 lb ft
Battery Cable-to-Battery | 17 N·m | 151 lb in
Battery Cable-to-Generator | 10 N·m | 89 lb in
Battery Case Bracket Stud and Nut | 9 N·m | 80 lb in
Belt Idler Pulley-to-Front Cover | 27 N·m | 20 lb ft
Belt Tensioner-to-Block | 30 N·m | 22 lb ft
Belt Tensioner Pulley | 30 N·m | 22 lb ft
Block Oil Gallery Plug | 30 N·m | 22 lb ft
Camshaft Bearing Cap-to-Head (LL0) | 14 N·m | 124 lb in
Camshaft Cover-to-Head (LL0) | 10 N·m | 89 lb in
Camshaft Sprockets-to-Camshafts | 100 N·m | 74 lb ft
Camshaft Thrust Bearing-to-Head (L24) | 25 N·m | 19 lb ft
Canister Assembly Band Clamp | 3.5 N·m | 31 lb in
Canister Purge Solenoid-to-Block | 30 N·m | 22 lb ft
Catalytic Convertor-to-Isolator | 25 N·m | 19 lb ft
Clutch Pressure Plate-to-Flywheel | 25 N·m | 19 lb ft
Connecting Rod Cap-to-Rod | Torque Angle
Control Arm to Knuckle - Lower | 75 N·m | 55 lb ft
Coolant/Cylinder Block Heater | 25 N·m | 19 lb ft
Coolant Drain-to-Plug/Block | 30 N·m | 22 lb ft
Cradle-to-Body | 205 N·m | 151 lb ft
Crankshaft Bearing Cap-to-Block | 50 N·m | 37 lb ft
Crankshaft Rear Oil Seal Carrier-to-Block | 11 N·m | 97 lb in
Crankshaft Vibration Damper/Pulley-to-Crankshaft | 215 N·m | 159 lb ft
Cylinder Head-to-Block (L24 and LL0) | Torque Angle
Cylinder Head Core Hole Plug Water Jacket (LL0) | 75 N·m | 55 lb ft
Deaeration Line-to-Rocker Cover (L24) | 10 N·m | 89 lb in
Deaeration Line Nut-to-Cylinder Head Fitting (L24) | 15 N·m | 133 lb in
Deaeration Line Clamp-to-Engine Lift Bracket (L24) | 11 N·m | 97 lb in
Deaeration Line Fitting-to-Cylinder Head | 8 N·m | 71 lb in
Engine Lift Bracket-to-Head (Front and Rear) - No A/C | 30 N·m | 22 lb ft
Engine Lift Bracket-to-Block - No A/C | 47 N·m | 35 lb ft
EGR Valve to Head/Intake Manifold - Bolt | 25 N·m | 19 lb ft
Exhaust Manifold Studs-to-Front Exhaust Pipe | 13 N·m | 115 lb in
Exhaust Manifold Studs-to-Head | 13 N·m | 115 lb in
Exhaust Manifold-to-Head (L24) | 22 N·m | 16 lb ft
Exhaust Manifold-to-Head (LL0) | 17 N·m | 150 lb in
Exhaust Pipe with Converter-to-Intermediate Pipe | 25 N·m | 19 lb ft
Exhaust Pipe Clamp-to-Support Bracket | 60 N·m | 44 lb ft
Exhaust Pipe (Front) to Manifold | 31 N·m | 23 lb ft
Exhaust Pipe Service Clamps | 41 N·m | 30 lb ft
Exhaust Pipe Support Bracket-to-Block | 45 N·m | 33 lb ft
Flexplate-to-Converter | 70 N·m | 52 lb ft
Flexplate-to-Crankshaft | 60 N·m | 44 lb ft
Flywheel/Flexplate Cover-to-Case | 10 N·m | 89 lb in
Flywheel-to-Crankshaft | 80 N·m | 59 lb ft
Front Cover-to-Block - Lower Center Bolt | 10 N·m | 89 lb in
Front Cover-to-Head/Block (Perimeter) and Top Center (DOHC) | 30 N·m | 22 lb ft
Front Engine Cover Studs (Torque Axis Engine Mount) | 10 N·m | 89 lb in
Fuel Feed Line Support Clip-to-Bracket | 4.5 N·m | 37 lb in
Fuel Filter/Pressure Regulator-to-Frame Rail | 8 N·m | 71 lb in
Fuel Line Shield-to-Underbody | 12 N·m | 9 lb ft
Fuel Line Support Bracket-to-Block and Intake | 30 N·m | 22 lb ft
Fuel Rail-to-Intake Manifold | 12 N·m | 9 lb ft
Fuel Tank Fill Hose-to-Clamp | 4 N·m | 35 lb in
Fuel Tank Fill Pipe-to-Underbody Rail | 8 N·m | 71 lb in
Fuel Tank Fill Pipe-to-Upper Bracket | 3.5 N·m | 31 lb in
Fuel Tank Straps-to-Body | 47 N·m | 35 lb ft
Fuel/Vapor Lines-to-Body | 4 N·m | 27 lb in
Generator to Block - Upper/Lower Bolt | 32 N·m | 24 lb ft
Heater Return Nipple-to-Block | 50 N·m | 37 lb ft
Heater Outlet-to-Intake Manifold (L24 and LL0) | 40 N·m | 30 lb ft
Ignition Module-to-Transaxle Case | 7 N·m | 62 lb in
Intake Manifold-to-Head (L24) | 30 N·m | 22 lb ft
Intake Manifold-to-Head (LL0) | 30 N·m | 22 lb ft
Intake Manifold Stud-to-Head (P/S Bracket, LL0) | 30 N·m | 22 lb ft
Intake Manifold Studs-to-Head | 13 N·m | 115 lb in
Intake Manifold Support Bracket-to-Block (LH, LL0/L24) | 30 N·m | 22 lb ft
Intake Manifold Support Bracket-to-Block (RH, LL0) | 55 N·m | 41 lb ft
Intake Manifold Support Bracket-to-Manifold (LL0) | 30 N·m | 22 lb ft
Motor Mount - Front-to-Block | 70 N·m | 52 lb ft
Motor Mount - Front-to-Front Cover (Torque Axis Engine Mount) | 50 N·m | 37 lb ft
Motor Mount - Rear-to-Block (LH and RH) | 48 N·m | 35 lb ft
Muffler Isolator Block-to-Body | 25 N·m | 19 lb ft
Muffler Strap around Muffler | 22 N·m | 16 lb ft
Oil Baffle Plate-to-Block (LL0) | 55 N·m | 41 lb ft
Oil Filter-to-Block | Gasket Contact and 3/4 to 1 Turn
Oil Filter Fitting-to-Block | 30 N·m | 22 lb ft
Oil Gallery Plug-to-Block | 30 N·m | 22 lb ft
Oil Level Indicator Tube-to-Block | 30 N·m | 22 lb ft
Oil Pan-to-Block | 9 N·m | 80 lb in
Oil Pan Drain Plug-to-Pan | 37 N·m | 27 lb ft
Oil Pickup Tube-to-Block | 15 N·m | 133 lb in
Oil Pipe Bracket-to-Block (L24) | 55 N·m | 41 lb ft
Oil Pipe Bracket-to-Block/Baffle Plate (LL0) | 15 N·m | 133 lb in
Oil Pump Cover-to-Front Cover | 11 N·m | 97 lb in
Power Steering Hoses-to-Gear and Pump | 27 N·m | 20 lb ft
Power Steering Pump Bracket-to-Block | 30 N·m | 22 lb ft
Power Steering Pump-to-Bracket | 30 N·m | 22 lb ft
Power Steering Pump Lower Support Bracket-to-Intake Manifold (LL0) | 30 N·m | 22 lb ft
Power Steering Pump Lower Support Bracket-to-Pump Bracket (LL0) | 30 N·m | 22 lb ft
Power Steering Pump Upper Support Bracket-to-Pump/Intake Manifold (LL0) | 30 N·m | 22 lb ft
Power Steering Return Hose Clamp-to-Pump | 2 N·m | 18 lb in
Radiator Support Brackets | 10 N·m | 89 lb in
Rocker Arm Cover-to-Head (L24) | 30 N·m | 22 lb ft
Rocker Arm Shaft-to-Head | 25 N·m | 19 lb ft
Sensor - Coolant Temperature-to-Head (PCM) | 8 N·m | 71 lb in
Sensor - Crankshaft Position-to-Block | 9 N·m | 80 lb in
Sensor - ESC Knock-to-Block | 15 N·m | 133 lb in
Sensor - Idle Air Control | 3.2 N·m | 28 lb in
Sensor - Induction Air-to-Intake Tube | 5 N·m | 44 lb in
Sensor - Map-to-Intake Manifold (LL0 and L24) | 3 N·m | 27 lb in
Sensor - Oil Pressure-to-Block | 45 N·m | 33 lb ft
Sensor - Oxygen-to-Exhaust Manifold | 45 N·m | 33 lb ft
Sensor - Throttle Position (TP) Switch | 2 N·m | 18 lb in
Sensor - Vehicle Speed | 26 N·m | 19 lb in
Spark Plug-to-Head | 27 N·m | 20 lb ft
Starter Motor-to-Block | 37 N·m | 27 lb ft
Steering Joint-to-Gear | 47 N·m | 35 lb ft
Stiffening Bracket-to-Engine/Transaxle Case/Exhaust Down Pipe | 54 N·m | 40 lb ft
Strut-to-Knuckle | 200 N·m | 148 lb ft
Thermostat Housing-to-Block | 30 N·m | 22 lb ft
Throttle Body-to-Air Intake Manifold (LL0 and L24) | 31 N·m | 23 lb ft
Timing Chain Fixed Guide-to-Block | 26 N·m | 19 lb ft
Timing Chain Fixed Guide-to-Head | 26 N·m | 19 lb ft
Timing Chain Pivot Guide-to-Head | 26 N·m | 19 lb ft
Timing Chain Tensioner-to-Block | 19 N·m | 168 lb in
Torque Converter-to-Flexplate | 70 N·m | 52 lb ft
Torque Strut-to-Cradle Bracket and Engine Front Mount-RH (Torque Axis Engine Mount) | 50 N·m | 37 lb ft
Transaxle Case to Block - Lower Bolts | 130 N·m | 98 lb ft
Transaxle Case to Block - Upper Studs | 90 N·m | 66 lb ft
Transaxle Flywheel/Flexplate Dust Cover to Transaxle | 10 N·m | 89 lb in
Transaxle Lower Mount-to-Cradle | 50 N·m | 37 lb ft
Transaxle Lower Mount-to-Transaxle | 31 N·m | 23 lb ft
Transaxle to Rear Mount-to-Transaxle | 30 N·m | 22 lb ft
Transaxle Torque Strut to Midrail | 50 N·m | 37 lb ft
Underbody Frame Rail Support (Fuel Line) | 12 N·m | 106 lb in
Upper Engine Mount-to-Front Cover and RH Frame Rail Bracket (Torque Axis Engine Mount) | 50 N·m | 37 lb ft
Water Pump-to-Block | 30 N·m | 22 lb ft
Water Pump Pulley-to-Water Pump Hub | 25 N·m | 19 lb ft
Wiring Harness Clamps-to-Block | 25 N·m | 19 lb ft
Wiring Harness PCM Ground-to-Block | 10 N·m | 89 lb in
Wiring Harness-to-Generator (Positive Terminal) | 10 N·m | 89 lb in
Wiring Harness-to-Starter (Positive Terminal) | 10 N·m | 89 lb in
Wiring Harness-to-Starter (Solenoid Terminal) | 4 N·m | 35 lb in
Wiring Harness-to-Transaxle Case/Engine Block (2) | 25 N·m | 18 lb ft