For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector from brake fluid level sensor.
2. Remove the brake fluid level sensor. Using needle nose pliers, carefully depress the retaining tabs on the end of the brake fluid level sensor (1) and press the sensor through the reservoir to remove.

### Installation Procedure

1. Place the brake fluid level sensor (1) into the reservoir, press into place to secure the sensor retaining tabs.
2. Connect the electrical connector to the brake fluid level sensor (1).