For 1990-2009 cars

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This tests for A/C compressor engagement. Ambient air temperature must be above 4°C (40°F) for the compressor to engage.

2. This tests for the blower motor functionality.

3. This tests if the A/C compressor function is inoperative.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: HVAC Schematics Connector End View Reference: HVAC Connector End Views DEFINITION: The temperature cannot be adjusted, or the cooling is insufficient during A/C operation.
1 | Did you perform the HVAC Diagnostics System Check? | Go to Step 2 | Go to Diagnostic System Check - HVAC Systems - Manual
2 | Important: The ambient air temperature must be above 4°C (40°F).

1. Turn OFF the ignition.
2. Inspect the A/C compressor for free rotation operation. Refer to Symptoms - HVAC Systems - Manual .
3. Start the engine.
4. Place the mode switch in Blend (face and feet) or Defrost.
5. Place the blower motor switch in the MAX position.
6. Place the air temperature switch in the coldest position.

Does the A/C compressor operate?

Go to Step 3

Go to HVAC Compressor Clutch Does Not Engage

3 |

1. Turn ON the ignition, with the engine OFF.
2. Place the mode switch in any position.
3. Place the blower switch in each speed position.

Does the blower motor operate in any of the speed positions?

Go to Step 4

Go to Blower Motor Inoperative

4 | Does the blower motor operate at the desired speeds? | Go to Step 5 | Go to Blower Motor Malfunction
5 |

1. Start the engine.
2. Place the blower motor switch in the maximum speed position.
3. Place the recirculation switch in the ON position.

Does the recirculation door move to the recirculation position?

Go to Step 6

Go to Air Recirculation Malfunction

6 | When the A/C is ON, does the customer concern occur? | Go to Step 7 | Go to Step 8
7 | Perform the refrigerant system performance test. Refer to Air Conditioning (A/C) System Performance Test in Heating, Ventilation and Air Conditioning. Did you find and correct the condition? | Go to Step 9 | Go to Step 8
8 | Inspect the air temperature door and linkage for the following conditions:

• | High effort to operate air temperature door.

• | Broken or binding linkages or air temperature door

• | An obstruction that prevents the air temperature door from operating within its full range of motion

• | Missing seals to the air temperature door

• | Misaligned seals to the air temperature door

Did you find and correct the condition?

Go to Step 9

Go to High or Low Temperature Control Effort in Heating, Ventilation and Air Conditioning

9 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2