For 1990-2009 cars

### Removal Procedure

1. Remove the cargo shade.
2. Remove the cargo cover side molding. Refer to Cargo Area Side Trim Panel Replacement .
3. Remove the rear seat upper shoulder belt fastener cover.
4. Remove the rear seat upper shoulder belt fastener to remove the shoulder belt.
5. Starting at the front edge of the molding, pull at the attaching clips to remove the molding assembly.

### Installation Procedure

1. Position the side molding at the attaching clips.
2. Secure the side molding by pushing gently at the clip locations.
3. Install the cargo cover molding assembly. Refer to Cargo Area Side Trim Panel Replacement .

Notice: Refer to Fastener Notice in the Preface section.

4. Install the upper shoulder belt fastener.

Tighten
Tighten the fasteners to 35 N·m (26 lb ft).

5. Snap the upper shoulder belt fastener cover into place.
6. Raise the rear seat back assembly.
7. Apply the weatherstrip over the front and rear of the side molding using a flat-bladed tool.
8. Install the cargo shade.
9. Function the shoulder belt assembly to assure the proper operation.