For 1990-2009 cars

### Removal Procedure

1. Remove the center trim plate by gently pulling rearward at the top to disengage the retaining clips.
2. Tilt the trim plate sideways and disconnect the traction control switch electrical connector.
3. Release the traction control switch lock tabs and push the switch through the front of the center trim plate.

### Installation Procedure

1. Push the traction through the front of the center trim plate until the switch snaps into the lock tabs.
2. Connect the traction control switch electrical connector.
3. Push the center trim plate into the instrument panel to engage the retaining clips.