For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement in Engine Controls 2.2L (L61).
2. Support the engine.
3. Remove the engine mount to bracket bolts.
4. Remove the engine mount to body bolts.
5. Remove the engine mount from the vehicle.
6. Remove the bolt the retains the mount to the engine mount body bracket.

Important: Retain the isolation pad for assembly.

7. Remove the mount from the mount bracket and isolation pad.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

Important: The isolation must be attached to the engine mount. Replace the isolation pad if necessary.

1. Assemble the engine mount , engine mount bracket and isolation pad.

Tighten
Tighten the engine mount to bracket bolt to 90 N·m (66 lb ft).

2. Install the engine mount to the vehicle. Hand tighten the bolts at this time.
3. Install the engine mount to engine bracket bolts.

Tighten

• | Tighten the engine mount to bracket bolts to 55 N·m (41 lb ft).

• | Tighten the engine mount to vehicle bolts to 55 N·m (41 lb ft).

4. Remove the engine support fixture.
5. Balance the engine mounts. Refer to Engine and Transmission Mount Balancing - All Mounts .
6. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement in Engine Controls 2.2L (L61).