For 1990-2009 cars

#### C102 Forward Lamp Harness to Right Headlamp Harness

Connector Part Information |

• | 15326829

• | 6-Way F GT 150 Sealed Series (BK)

Connector Part Information

• | 15326833

• | 6-Way M GT 150 Selaed Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | OG | 140 | Battery Positive Voltage | A | OG | 140 | Battery Positive Voltage
B | BN | 9 | Park Lamp Supply Voltage | B | BN | 9 | Park Lamp Supply Voltage
C | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | C | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
D | PK | 1200 | High Beam Switched Ground | D | PK | 1200 | High Beam Switched Ground
E | L-BU | 1201 | Low Beam Switched Ground | E | L-BU | 1201 | Low Beam Switched Ground
F | BK | 150 | Ground | F | BK | 150 | Ground

#### C103 Forward Lamp Harness to Left Headlamp Harness

Connector Part Information |

• | 15326829

• | 6-Way F GT 150 Sealed Series (BK)

Connector Part Information

• | 15326833

• | 6-Way M GT 150 Selaed Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | OG | 40 | Battery Positive Voltage | A | OG | 40 | Battery Positive Voltage
B | BN | 9 | Park Lamp Supply Voltage | B | BN | 9 | Park Lamp Supply Voltage
C | L-BU | 14 | Left Turn Signal Lamps Supply Voltage | C | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
D | PK | 1200 | High Beam Switched Ground | D | PK | 1200 | High Beam Switched Ground
E | L-BU | 1201 | Low Beam Switched Ground | E | L-BU | 1201 | Low Beam Switched Ground
F | BK | 150 | Ground | F | BK | 150 | Ground

#### C150 Engine Harness to Injector Jumper (3.0L)

| --
--- | ---
Connector Part Information |

• | 15354678

• | 10-Way F (BK)

Connector Part Information

• | 12186711

• | 10-Way M (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BK | 1744 | Fuel Injector 1 Control | 1 | BK | 1744 | Fuel Injector 1 Control
2 | GN/BK | 1745 | Fuel Injector 2 Control | 2 | GN/BK | 1745 | Fuel Injector 2 Control
3 | PK/BK | 1746 | Fuel Injector 3 Control | 3 | PK/BK | 1746 | Fuel Injector 3 Control
4 | BU/BK | 844 | Fuel Injector 4 Control | 4 | BU/BK | 844 | Fuel Injector 4 Control
5 | BK/WH | 845 | Fuel Injector 5 Control | 5 | BK/WH | 845 | Fuel Injector 5 Control
6 | YE/BK | 846 | Fuel Injector 6 Control | 6 | YE/BK | 846 | Fuel Injector 6 Control
7 | -- | -- | Not Used | 7 | -- | -- | Not Used
8 | OG | 2640 | Ignition 1 Voltage | 8 | OG | 2640 | Ignition 1 Voltage

#### C150 Inline Engine Harness to Injector Harness (2.2L)

Connector Part Information |

• | 15326835

• | 8-Way F GT 150 Series (BK)

Connector Part Information

• | 15326840

• | 8-Way M GT 150 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BK | 1744 | Injector 1 Control | A | BK | 1744 | Injector 1 Control
B | L-GN/BK | 1745 | Injector 2 Control | B | L-GN/BK | 1745 | Injector 2 Control
C | PK/BK | 1746 | Injector 3 Control | C | PK/BK | 1746 | Injector 3 Control
D | L-BU/BK | 844 | Injector 4 Control | D | L-BU/BK | 844 | Injector 4 Control
E | PK | 139 | Ignition 1 Voltage | E | PK | 139 | Ignition 1 Voltage
F | OG/BK | 469 | Low Reference | F | OG/BK | 469 | Low Reference
G | GN | 432 | MAP Sensor Signal | G | L-GN | 432 | MAP Sensor Signal
H | GY | 2704 | 5 Volt Reference | H | GY | 2704 | 5 Volt Reference

#### C198 Engine Harness to I/P Harness (3.0L Late Production)

Connector Part Information |

• | 15326849

• | 12-Way F GT 150 Series (BK)

Connector Part Information

• | 15326854

• | 12-Way M GT 150 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | D-BU | 84 | Cruise Control Set/Coast Switch Signal | A1 | D-BU | 84 | Cruise Control Set/Coast Switch Signal
B | BK | 2759 | Low Reference | A2 | BK | 2759 | Low Reference
C | L-BU | 1162 | APP Sensor 2 Signal | A3 | L-BU | 1162 | APP Sensor 2 Signal
D | BN | 86 | Cruise Control Release Signal | A4 | BN | 86 | Cruise Control Release Signal
E | BN | 1271 | Low Reference | A5 | BN | 1271 | Low Reference
F | GY | 397 | Cruise Control On Switch Signal | A6 | GY | 397 | Cruise Control On Switch Signal
G | D-BU | 1161 | APP Sensor 1 Signal | A7 | D-BU | 1161 | APP Sensor 1 Signal
H | TN | 1274 | 5 Volt Reference | A8 | TN | 1274 | 5 Volt Reference
J | WH/BK | 1164 | 5 Volt Reference | B1 | WH/BK | 1164 | 5 Volt Reference
K | PU | 1319 | Engine/Radio Serial Data K-Line | B2 | PU | 1319 | Engine/Radio Serial Data K-Line
L | GY | 2709 | 5 Volt Reference | B3 | GY | 2709 | 5 Volt Reference
M | WH | 1310 | EVAP Canister Vent Solenoid Control | B4 | WH | 1310 | EVAP Canister Vent Solenoid Control

#### C199 Engine Harness to I/P Harness (2.2L)

Connector Part Information |

• | 15366099

• | 24-Way F GT 150/280 Series (BK)

Connector Part Information

• | 15336173

• | 24-Way M GT 150/280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1 | BK/WH | 451 | Ground | A1 | BK/WH | 451 | Ground
A2 | WH | 776 | Transmission Range Switch Signal P (A/T) | A2 | BN/WH | 776 | Transmission Range Switch Signal P (A/T)
BN/WH | 379 | CPP Switch Signal (M/T) | PU | 379 | CPP Switch Signal (M/T)
A3 | PU | 30 | Fuel Level Sensor Signal | A3 | PU | 30 | Fuel Level Sensor Signal
A4 | YE | 5 | Crank Voltage (A/T) | A4 | YE | 5 | Crank Voltage (A/T)
PU | 6 | Starter Solenoid Crank Voltage (M/T) | PU | 6 | Starter Solenoid Crank Voltage (M/T)
A5 | WH | 1310 | EVAP Canister Vent Solenoid Control | A5 | WH | 1310 | EVAP Canister Vent Solenoid Control
A6 | BK/WH | 451 | Ground | A6 | BK/WH | 451 | Ground
A7 | D- GN/WH | 817 | Vehicle Speed Signal | A7 | D- GN/WH | 817 | Vehicle Speed Signal
A8 | L-BU/BK | 396 | Cruise Control Engaged Signal | A8 | L-BU/BK | 396 | Cruise Control Engaged Signal
B1 | D- GN | 890 | Fuel Tank Pressure Sensor Signal | B1 | D- GN | 890 | Fuel Tank Pressure Sensor Signal
B2 | BK | 2759 | Low Reference | B2 | BK | 2759 | Low Reference
B3 | GY | 2709 | 5 Volt Reference | B3 | GY | 2709 | 5 Volt Reference
B4 | YE | 343 | Accessory Voltage | B4 | YE | 343 | Accessory Voltage
B5 | PU | 1807 | Class 2 Serial Data | B5 | PU | 1807 | Class 2 Serial Data
B6 | BN | 882 | Right Rear Wheel Speed Sensor Signal (w/ ABS) | B6 | BN | 882 | Right Rear Wheel Speed Sensor Signal (w/ ABS)
BN | 872 | Right Rear Wheel Speed Sensor Signal (w/o ABS) | BN | 872 | Right Rear Wheel Speed Sensor Signal (w/o ABS)
B7 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference (w/ ABS) | B7 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference (w/ ABS)
WH | 833 | Right Front Wheel Speed Sensor Low Reference (w/o ABS) | WH | 833 | Right Front Wheel Speed Sensor Low Reference (w/o ABS)
B8 | D- GN | 83 | Cruise Control Inhibit Signal | B8 | D- GN | 83 | Cruise Control Inhibit Signal
C1 | YE | 772 | Transmission Range Switch Signal B (A/T) | C1 | YE | 772 | Transmission Range Switch Signal B (A/T)
WH | 1909 | Right Front Wheel Speed Sensor Signal (M/T) | WH | 1909 | Right Front Wheel Speed Sensor Signal (M/T)
C2 | L-BU | 1788 | Traction Control Switch Signal | C2 | L-BU | 1788 | Traction Control Switch Signal
C3 | L-BU | 1276 | ABS Serial Data K-Line | C3 | L-BU | 1276 | ABS Serial Data K-Line
C4 | PU | 92 | Windshield Wiper Motor High Speed | C4 | PU | 92 | Windshield Wiper Motor High Speed
C5 | D- GN | 95 | Windshield Washer Switch Signal | C5 | D- GN | 95 | Windshield Washer Switch Signal
C6 | BK | 884 | Left Rear Wheel Speed Sensor Signal | C6 | BK | 884 | Left Rear Wheel Speed Sensor Signal
C7 | RD | 885 | Left Rear Wheel Speed Sensor Low Reference | C7 | RD | 885 | Left Rear Wheel Speed Sensor Low Reference
C8 | PU | 1807 | Class 2 Serial Data | C8 | PU | 1807 | Class 2 Serial Data

#### C199 Engine Harness to I/P Harness (3.0L Early Production)

Connector Part Information |

• | 15336418

• | 38-Way F GT 150/280 Series (BK)

Connector Part Information

• | 15317380

• | 38-Way M GT 150/280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1 | GY/BK | 87 | Cruise Control Resume/Accel Switch Signal | A1 | GY/BK | 87 | Cruise Control Resume/Accel Switch Signal
A2 | WH | 776 | Transmission Range Switch Signal P | A2 | WH | 776 | Transmission Range Switch Signal P
A3 | PU | 30 | Fuel Level Sensor Signal | A3 | PU | 30 | Fuel Level Sensor Signal
A4 | YE | 5 | Crank Voltage | A4 | YE | 5 | Crank Voltage
A5 | PU | 1319 | Engine/Radio Serial Data K-Line | A5 | PU | 1319 | Engine/Radio Serial Data K-Line
A6 | TN | 2501 | CAN Low | A6 | TN | 2501 | CAN Low
A7 | TN/WH | 2500 | CAN High | A7 | TN/WH | 2500 | CAN High
A8 | D- GN | 890 | Fuel Tank Pressure Sensor Signal | A8 | D- GN | 890 | Fuel Tank Pressure Sensor Signal
B1 | BK | 2759 | Low Reference | B1 | BK | 2759 | Low Reference
B2 | GY | 2709 | 5 Volt Reference | B2 | GY | 2709 | 5 Volt Reference
B3 | BN | 882 | Right Rear Wheel Speed Sensor Signal | B3 | BN | 882 | Right Rear Wheel Speed Sensor Signal
B4 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference | B4 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference
TN | 833 | Right Front Wheel Speed Sensor Low Reference
B5 | D- BLU | 84 | Cruise Control Set/Coast Switch Signal | B5 | D- BLU | 84 | Cruise Control Set/Coast Switch Signal
B6 | YE | 343 | Accessory Voltage | B6 | YE | 343 | Accessory Voltage
B7 | -- | -- | Not Used | B7 | -- | -- | Not Used
B8 | BK | 2759 | Low Reference | B8 | BK | 2759 | Low Reference
B9 | L-BU | 1162 | APP Sensor 2 Signal | B9 | L-BU | 1162 | APP Sensor 2 Signal
B10 | BN | 86 | Cruise Control Release Signal | B10 | BN | 86 | Cruise Control Release Signal
B11 | BN | 1271 | Low Reference | B11 | BN | 1271 | Low Reference
B12 | GY | 397 | Cruise Control On Switch Signal | B12 | GY | 397 | Cruise Control On Switch Signal
C1 | D- BLU | 1161 | APP Sensor 1 Signal | C1 | D- BLU | 1161 | APP Sensor 1 Signal
C2 | TN | 1274 | 5 Volt Reference | C2 | TN | 1274 | 5 Volt Reference
C3 | WH/BK | 1164 | 5 Volt Reference | C3 | WH/BK | 1164 | 5 Volt Reference
C4 | -- | -- | Not Used | C4 | -- | -- | Not Used
C5 | PU | 1319 | Engine/Radio Serial Data K-Line | C5 | PU | 1319 | Engine/Radio Serial Data K-Line
C6 | PU | 92 | Windshield Wiper Motor High Speed | C6 | PU | 92 | Windshield Wiper Motor High Speed
C7 | D- GN | 95 | Windshield Washer Switch Signal | C7 | D- GN | 95 | Windshield Washer Switch Signal
C8 | GY | 2709 | 5 Volt Reference | C8 | GY | 2709 | 5 Volt Reference
C9 | L-BU | 1788 | Traction Control Switch Signal | C9 | L-BU | 1788 | Traction Control Switch Signal
C10 | WH | 2192 | Traction Ready Indicator Control | C10 | WH | 2192 | Traction Ready Indicator Control
C11 | L-GN | 867 | ABS Indicator Failure Control | C11 | L-GN | 867 | ABS Indicator Failure Control
C12 | L-BU | 832 | Traction Control Active Signal | C12 | L-BU | 832 | Traction Control Active Signal
D1 | L-BU | 1276 | ABS Serial Data K-Line | D1 | L-BU | 1276 | ABS Serial Data K-Line
D2 | BK | 884 | Left Rear Wheel Speed Sensor Signal | D2 | BK | 884 | Left Rear Wheel Speed Sensor Signal
D3 | RD | 885 | Left Rear Wheel Speed Sensor Low Reference | D3 | RD | 885 | Left Rear Wheel Speed Sensor Low Reference
D4-D5 | -- | -- | Not Used | D4-D5 | -- | -- | Not Used
D6 | WH | 1310 | EVAP Canister Vent Solenoid Control | D6 | WH | 1310 | EVAP Canister Vent Solenoid Control
D7 | BK/WH | 451 | Ground | D7 | BK/WH | 451 | Ground
D8 | YE | 772 | Transmission Range Switch Signal B | D8 | YE | 772 | Transmission Range Switch Signal B

#### C199 Engine Harness to I/P Harness (3.0L Late Production)

Connector Part Information |

• | 15366099

• | 24-Way F GT 150/280 Series (BK)

Connector Part Information

• | 15336173

• | 24-Way M GT 150/280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1 | GY/BK | 87 | Cruise Control Resume/Accel Switch Signal | A1 | GY/BK | 87 | Cruise Control Resume/Accel Switch Signal
A2 | WH | 776 | Transmission Range Switch Signal P | A2 | WH | 776 | Transmission Range Switch Signal P
A3 | PU | 30 | Fuel Level Sensor Signal | A3 | PU | 30 | Fuel Level Sensor Signal
A4 | YE | 5 | Crank Voltage | A4 | YE | 5 | Crank Voltage
A5 | PU | 1319 | Engine/Radio Serial Data K-Line | A5 | PU | 1319 | Engine/Radio Serial Data K-Line
A6 | TN | 2501 | CAN Low | A6 | TN | 2501 | CAN Low
A7 | TN/WH | 2500 | CAN High | A7 | TN/WH | 2500 | CAN High
A8 | D- GN | 890 | Fuel Tank Pressure Sensor Signal | A8 | D- GN | 890 | Fuel Tank Pressure Sensor Signal
B1 | BK | 2759 | Low Reference | B1 | BK | 2759 | Low Reference
B2 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference | B2 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference
B3 | BN | 882 | Right Rear Wheel Speed Sensor Signal | B3 | BN | 882 | Right Rear Wheel Speed Sensor Signal
B4 | PU | 92 | Windshield Wiper Motor High Speed | B4 | PU | 92 | Windshield Wiper Motor High Speed
B5 | YE | 343 | Accessory Voltage | B5 | YE | 343 | Accessory Voltage
B6 | L-BU | 1788 | Traction Control Switch Signal | B6 | L-BU | 1788 | Traction Control Switch Signal
B7 | WH | 2192 | Traction Ready Indicator Control | B7 | WH | 2192 | Traction Ready Indicator Control
B8 | GY | 2709 | 5 Volt Reference | B8 | GY | 2709 | 5 Volt Reference
C1 | BK/WH | 451 | Ground | C1 | BK/WH | 451 | Ground
C2 | L-GN | 867 | ABS Indicator Failure Control (w/ ABS) | C2 | L-GN | 867 | ABS Indicator Failure Control (w/ ABS)
C3 | L-BU | 832 | Traction Control Active Signal (w/ ABS) | C3 | L-BU | 832 | Traction Control Active Signal (w/ ABS)
C4 | L-BU | 1276 | ABS Serial Data K-Line (w/ ABS) | C4 | L-BU | 1276 | ABS Serial Data K-Line (w/ ABS)
C5 | D-GN | 95 | Windshield Washer Switch Signal | C5 | D-GN | 95 | Windshield Washer Switch Signal
C6 | OG | 885 | Left Rear Wheel Speed Sensor Low Reference (w/ ABS) | C6 | OG | 885 | Left Rear Wheel Speed Sensor Low Reference (w/ ABS)
C7 | TN | 884 | Windshield Washer Switch Signal (w/ ABS) | C7 | TN | 884 | Windshield Washer Switch Signal (w/ ABS)
C8 | YE | 772 | Transmission Range Switch Signal B | C8 | YE | 772 | Transmission Range Switch Signal B

#### C200 Body Harness to Headliner- Front

Connector Part Information |

• | 15336888

• | 12-Way F GT 150/280 Series (BK)

Connector Part Information

• | 15354991

• | 12 Way M GT 150/280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | OG | 1732 | Courtesy Lamps Supply Voltage | A | OG | 1732 | Courtesy Lamps Supply Voltage
B | OG | 1732 | Courtesy Lamps Supply Voltage | B | OG | 1732 | Courtesy Lamps Supply Voltage
C | L-BU | 20 | Stop Lamp Switch Signal | C | L-BU | 20 | Stop Lamp Switch Signal
OG | 1732 | Courtesy Lamps Supply Voltage (Wagon) | OG | 1732 | Courtesy Lamps Supply Voltage (Wagon)
D | YE | 143 | Accessory Voltage (Sedan) | D | YE | 143 | Accessory Voltage (Sedan)
E | RD | 402 | Battery Positive Voltage | E | RD | 402 | Battery Positive Voltage
F | WH | 156 | Courtesy Lamp Low Control | F | WH | 156 | Courtesy Lamp Low Control
G | -- | -- | Not Used | G | -- | -- | Not Used
H | BK | 450 | Ground | H | BK | 450 | Ground
J-M | -- | -- | Not Used | J-M | -- | -- | Not Used

#### C201 Body Harness to Audio Amplifier Harness

Connector Part Information |

• | 12064752

• | 6-Way F Metri-Pack 280 Series (BK)

Connector Part Information

• | 12064754

• | 6-Way M Metri-Pack 280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BLU | 346 | Subwoofer Speaker Output (+) | A | BLU | 346 | Subwoofer Speaker Output (+)
B | GN | 1794 | Subwoofer Speaker Output (-) | B | GN | 1794 | Subwoofer Speaker Output (-)
C | OG | 1340 | Battery Positive Voltage | C | OG | 1340 | Battery Positive Voltage
D | BK | 450 | Ground | D | BK | 450 | Ground
E-F | -- | -- | Not Used | E-F | -- | -- | Not Used

#### C204 Body Harness to I/P (RH) Harness (w/ UE1)

Connector Part Information |

• | 15317325

• | 22-Way F GT 150/280 Series (L-GY)

Connector Part Information

• | 15317322

• | 22-Way M GT 150/280 Series (L-GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1 | WH | 156 | Courtesy Lamp Low Control | A1 | WH | 156 | Courtesy Lamp Low Control
A2 | D-GN/WH | 368 | Remote Radio Right Audio Signal | A2 | D-GN/WH | 368 | Remote Radio Right Audio Signal
A3 | BARE | 814 | Drain Wire | A3 | BARE | 814 | Drain Wire
A4 | BK/WH | 746 | Right Front Door Ajar Switch Signal | A4 | BK/WH | 746 | Right Front Door Ajar Switch Signal
BK/WH | 746 | Right Front Door Ajar Switch Signal |  | BK/WH | 746 | Right Front Door Ajar Switch Signal
A5 | RD/BK | 744 | Rear Compartment Lid Adjar Switch | A5 | RD/BK | 744 | Rear Compartment Lid Adjar Switch
A6 | GY | 382 | Trunk Release Enable Relay Switch Supply Voltage | A6 | GY | 382 | Trunk Release Enable Relay Switch Supply Voltage
A7 | BK/WH | 746 | Right Front Door Ajar Switch Signal | A7 | BK/WH | 746 | Right Front Door Ajar Switch Signal
A8 | OG | 1732 | Courtesy Lamps Supply Voltage | A8 | OG | 1732 | Courtesy Lamps Supply Voltage
A9 | BN/WH | 367 | Remote Radio Left Audio Signal | A9 | BN/WH | 367 | Remote Radio Left Audio Signal
A10 | YE/BK | 693 | Cellular Telephone Mute Signal | A10 | YE/BK | 693 | Cellular Telephone Mute Signal
A11 | BK/WH | 372 | Remote Radio Audio Output (-) | A11 | BK/WH | 372 | Remote Radio Audio Output (-)
B1 | -- | -- | Not Used | B1 | -- | -- | Not Used
B2 | D-BU | 1363 | Seat Belt Switch - Left - Low Reference | B2 | D-BU | 1363 | Seat Belt Switch - Left - Low Reference
B3 | BK/WH | 238 | Seat Belt Switch - Left | B3 | BK/WH | 238 | Seat Belt Switch - Left
B4 | OG | 1732 | Courtesy Lamps Supply Voltage | B4 | OG | 1732 | Courtesy Lamps Supply Voltage
OG | 1732 | Courtesy Lamps Supply Voltage |  | OG | 1732 | Courtesy Lamps Supply Voltage
B5 | D-GN | 117 | Right Front Speaker Output (-) | B5 | D-GN | 117 | Right Front Speaker Output (-)
B6 | L-GN | 200 | Right Front Speaker Output (+) | B6 | L-GN | 200 | Right Front Speaker Output (+)
B7 | PU | 1807 | Class 2 Serial Data | B7 | PU | 1807 | Class 2 Serial Data
PU | 1807 | Class 2 Serial Data | Class 2 Serial Data
B8 | D-BU | 46 | Right Rear Speaker Output (+) | B8 | D-BU | 46 | Right Rear Speaker Output (+)
B9 | BK | 650 | Ground | B9 | BK | 650 | Ground
B10 | OG | 1340 | Battery Positive Voltage | B10 | OG | 1340 | Battery Positive Voltage
B11 | L-BU | 115 | Right Rear Speaker Output (-) | B11 | L-BU | 115 | Right Rear Speaker Output (-)

#### C204 Body Harness to I/P (RH) Harness (w/o UE1)

Connector Part Information |

• | 12129430

• | 16-Way F GT 150/280 Series (WH)

Connector Part Information

• | 12129429

• | 16-Way M GT 150/280 Series (WH)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | D- BLU | 46 | Right Rear Speaker Output (+) | A | D- BLU | 46 | Right Rear Speaker Output (+)
B | L-BU | 115 | Right Rear Speaker Output (-) | B | L-BU | 115 | Right Rear Speaker Output (-)
C | L-GN | 200 | Right Front Speaker Output (+) | C | L-GN | 200 | Right Front Speaker Output (+)
D | D- GN | 117 | Right Front Speaker Output (-) | D | D- GN | 117 | Right Front Speaker Output (-)
E | BK/WH | 238 | Seat Belt Switch - Left | E | BK/WH | 238 | Seat Belt Switch - Left
F | D- BLU | 1363 | Seat Belt Switch - Left - Low Reference | F | D- BLU | 1363 | Seat Belt Switch - Left - Low Reference
G | OG | 1732 | Courtesy Lamps Supply Voltage | G | OG | 1732 | Courtesy Lamps Supply Voltage
H | OG | 1732 | Courtesy Lamps Supply Voltage | H | -- | -- | Courtesy Lamps Supply Voltage
J | WH | 156 | Courtesy Lamp Low Control | J | WH | 156 | Courtesy Lamp Low Control
K | RD/WH | 744 | Rear Compartment Lid Adjar Switch | K | RD/BK | 744 | Rear Compartment Lid Adjar Switch
L | BK/WH | 746 | Right Front Door Ajar Switch Signal | L | BK/WH | 746 | Right Front Door Ajar Switch Signal
M | BK/WH | 746 | Right Front Door Ajar Switch Signal | M | BK/WH | 746 | Right Front Door Ajar Switch Signal
N | GY | 382 | Trunk Release Enable Relay Switch Supply Voltage | N | GY | 382 | Trunk Release Enable Relay Switch Supply Voltage
P-S | -- | -- | Not Used | P-S | -- | -- | Not Used

#### C205 I/P Harness to HVAC Jumper (w/ C68)

Connector Part Information |

• | 15336205

• | 12-Way F GT 150/280 Series (BK)

Connector Part Information

• | 15336209

• | 12-Way M GT 150/280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | YE | 268 | Ignition 3 Voltage | A | OG/TN | YE | Ignition 3 Voltage
B | TN | 683 | Rear Defog Indicator Supply Voltage | B | OG/YE | TN | Rear Defog Indicator Supply Voltage
C | BK | 550 | Ground | c | BK | BK | Ground
D | YE | 61 | Low Reference | D | L-GN/YE | YE | Low Reference
E | L-BU/BK | 590 | Sunload Sensor Signal | E | BN/L-BU | L-BU/BK | Sunload Sensor Signal
F | BK | 550 | Ground | F | BK | BK | Ground
G | GY | 8 | Instrument Panel Lamp Supply Voltage | G | GY | GY | Instrument Panel Lamp Supply Voltage
H | BN | 641 | Ignition 3 Voltage | H | BN | BN | Ignition 3 Voltage
J | PU | 1807 | Class 2 Serial Data | J | L-BU/PU | PU | Class 2 Serial Data
K | PU | 1807 | Class 2 Serial Data | K | TN/PU | PU | Class 2 Serial Data
L | OG | 1640 | Battery Positive Voltage | L | OG | OG | Battery Positive Voltage
M | BK | 476 | Low Reference | M | BK | 476 | Low Reference
BK | 476 | Low Reference

#### C205 I/P Harness to HVAC Jumper (w/o C68)

Connector Part Information |

• | 15336888

• | 12-Way F GT 150/280 Series (BK)

Connector Part Information

• | 15336891

• | 12-Way M GT 150/280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | OG | 52 | Blower Motor High Control | A | OG | 52 | Blower Motor High Control
B | OG | 52 | Blower Motor High Control | B | OG | 52 | Blower Motor High Control
C | BK | 550 | Ground | c | BK | 550 | Ground
D | L-GN | 66 | A/C Request Signal | D | L-GN | 66 | A/C Request Signal
E | YE | 268 | Ignition 3 Voltage | E | YE | 268 | Ignition 3 Voltage
F | BK | 550 | Ground | F | BK | 550 | Ground
G | GY | 8 | Instrument Panel Lamp Supply Voltage | G | GY | 8 | Instrument Panel Lamp Supply Voltage
H | BN | 641 | Ignition 3 Voltage | H | BN | 641 | Ignition 3 Voltage
J | L-BU | 292 | Rear Defog Switch Signal | J | L-BU | 292 | Rear Defog Switch Signal
K | TN | 683 | Rear Defog Indicator Supply Voltage | K | TN | 683 | Rear Defog Indicator Supply Voltage
L | -- | -- | Not Used | L | -- | -- | Not Used

#### C207 Body Harness to I/P Harness

Connector Part Information |

• | 15336888

• | 12-Way F GT 150/280 Series (BK)

Connector Part Information

• | 15336891

• | 12-Way M GT 150/280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | GY | 2709 | 5 Volt Reference | A | GY | 2709 | 5 Volt Reference
B | TN | 201 | Left Front Speaker Output (+) | B | TN | 201 | Left Front Speaker Output (+)
C | D- GN | 890 | Fuel Tank Pressure Sensor Signal | C | D- GN | 890 | Fuel Tank Pressure Sensor Signal
D | BK | 884 | Left Rear Wheel Speed Sensor Signal | D | BK | 884 | Left Rear Wheel Speed Sensor Signal
E | YE | 182 | Heated Seat Control Module Inhibit Signal | E | YE | 182 | Heated Seat Control Module Inhibit Signal
F | WH | 883 | Right Rear Wheel Speed Sensor Low Reference | F | WH | 883 | Right Rear Wheel Speed Sensor Low Reference
G | GY | 118 | Left Front Speaker Output (-) | G | GY | 118 | Left Front Speaker Output (-)
H | BN | 882 | Right Rear Wheel Speed Sensor Signal | H | BN | 882 | Right Rear Wheel Speed Sensor Signal
J | RD | 885 | Left Rear Wheel Speed Sensor Low Reference | J | RD | 885 | Left Rear Wheel Speed Sensor Low Reference
K | PK | 1501 | Driver Heated Seat High/Low Signal | K | PK | 1501 | Driver Heated Seat High/Low Signal
L | BN | 199 | Left Rear Speaker Output (+) | L | BN | 199 | Left Rear Speaker Output (+)
M | YE | 116 | Left Rear Speaker Output (-) | M | YE | 116 | Left Rear Speaker Output (-)

#### C215 Inflatable Restraint I/P Module to I/P Harness

Connector Part Information |

• | 12077921

• | 2-Way F Metri-Pack 280 Series (YE)

Connector Part Information

• | 12186799

• | 2-Way M Metri-Pack 280 Series (YE)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | WH/BK | 1403 | I/P Module - High Control | A | WH/BK | 1403 | I/P Module - High Control
B | D- GN/WH | 1404 | I/P Module - Low Control | B | D- GN/WH | 1404 | I/P Module - Low Control

#### C220 I/P Harness to Audio Amplifier Harness

Connector Part Information |

• | 12110088

• | 24-Way F Micro-Pack 100 (GY)

Connector Part Information

• | 15305213

• | 24-Way M Micro-Pack 100 Series (GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A1-A7 | -- | -- | Not Used | A1-A7 | -- | -- | Not Used
A8 | BN | 199 | Left Rear Speaker Output (+) | A8 | BN | 199 | Left Rear Speaker Output (+)
A9 | YE | 116 | Left Rear Speaker Output (-) | A9 | YE | 116 | Left Rear Speaker Output (-)
A10 | GN | 117 | Right Front Speaker Output (-) | A10 | GN | 117 | Right Front Speaker Output (-)
A11 | GN | 200 | Right Front Speaker Output (+) | A11 | GN | 200 | Right Front Speaker Output (+)
A12 | BK | 550 | Ground | A12 | BK | 550 | Ground
B1 | OG | 440 | Battery Positive Voltage | B1 | OG | 440 | Battery Positive Voltage
B2 | YE | 43 | Accessory Voltage | B2 | YE | 43 | Accessory Voltage
B3 | OG | 2140 | Battery Positive Voltage | B3 | OG | 2140 | Battery Positive Voltage
B4 | GY | 8 | Instrument Panel Lamp Supply Voltage | B4 | GY | 8 | Instrument Panel Lamp Supply Voltage
B5-B7 | -- | -- | Not Used | B5-B7 | -- | -- | Not Used
B8 | TN | 201 | Left Front Speaker Output (+) | B8 | TN | 201 | Left Front Speaker Output (+)
B9 | GY | 118 | Left Front Speaker Output (-) | B9 | GY | 118 | Left Front Speaker Output (-)
B10 | BLU | 115 | Right Rear Speaker Output (-) | B10 | BLU | 115 | Right Rear Speaker Output (-)
B11 | BLU | 46 | Right Rear Speaker Output (+) | B11 | BLU | 46 | Right Rear Speaker Output (+)
B12 | BN | 9 | Park Lamp Supply Voltage | B12 | BN | 9 | Park Lamp Supply Voltage

#### C301 I/P to Console Jumper

Connector Part Information |

• | 12064752

• | 6-Way F Metri-Pack 280 Series (BK)

Connector Part Information

• | 12064754

• | 6-Way M Metri-Pack 280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | -- | -- | Not Used | A | GY | 8 | Not Used
B | OG | 2240 | Battery Positive Voltage | B | OG | 2240 | Battery Positive Voltage
C | BK | 350 | Ground | C | BK | 350 | Ground
BK | 550 | Ground | BK | 550 | Ground
D | OG | 1740 | Battery Positive Voltage | D | OG | 1740 | Battery Positive Voltage
E-F | -- | -- | Not Used | E-F | -- | -- | Not Used

#### C305 Body Harness to Driver Seat

Connector Part Information |

• | 15318082

• | 8 Way F (BK)

Connector Part Information

• | 15397088

• | 8-Way M (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PK | 1501 | Driver Heated Seat High/Low Signal | 1 | PK | 1501 | Driver Heated Seat High/Low Signal
2 | YE | 182 | Heated Seat Control Module Inhibit Signal | 2 | YE | 182 | Heated Seat Control Module Inhibit Signal
3 | BN | 141 | Ignition 3 Voltage | 3 | BN | 141 | Ignition 3 Voltage
4 | BK | 450 | Ground | 4 | BK | 450 | Ground
5 | OG | 640 | Batery Positive Voltage | 5 | OG | 640 | Batery Positive Voltage
6 | BK | 450 | Ground | 6 | BK | 450 | Ground
7 | D- BLU | 1363 | Seat Belt Switch - Left - Low Reference | 7 | D- BLU | 1363 | Seat Belt Switch - Left - Low Reference
8 | BK/WH | 238 | Seat Belt Switch - Left | 8 | BK/WH | 238 | Seat Belt Switch - Left

#### C306 Body Harness to Front Passenger Seat

Connector Part Information |

• | 15318082

• | 8 Way F (BK)

Connector Part Information

• | 15397088

• | 8-Way M (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | PK/BK | 1503 | Passenger Heated Seat High/Low Signal | 1 | PK/BK | 1503 | Passenger Heated Seat High/Low Signal
2 | L-GN | 559 | Heated Seat Control Module Inhibit Signal | 2 | L-GN | 559 | Heated Seat Control Module Inhibit Signal
3 | BN | 141 | Ignition 3 Voltage | 3 | BN | 141 | Ignition 3 Voltage
4 | BK | 450 | Ground | 4 | BK | 450 | Ground
5-8 | -- | -- | Not Used | 5-8 | -- | -- | Not Used

#### C406 Body Harness to Fuel Tank

Connector Part Information |

• | 15326835

• | 8-Way F GT 150 Series (BK)

Connector Part Information

• | 15326840

• | 8-Way M GT 150 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | GY | 120 | Fuel Pump Supply Voltage | A | GY | 120 | Fuel Pump Supply Voltage
B | BK | 650 | Ground | B | BK | 650 | Ground
C | BK | 2759 | Low Reference | C | BK | 2759 | Low Reference
D | -- | -- | Not Used | D | -- | -- | Not Used
E | D- GN | 890 | Fuel Tank Pressure Sensor Signal | E | D- GN | 890 | Fuel Tank Pressure Sensor Signal
F | GY | 2709 | 5 Volt Reference | F | GY | 2709 | 5 Volt Reference
G | BK | 2759 | Low Reference | G | BK | 2759 | Low Reference
H | PU | 30 | Fuel Level Sensor Signal | H | PU | 30 | Fuel Level Sensor Signal

#### C407 Body Harness to EVAP Solenoid Jumper

Connector Part Information |

• | 15326801

• | 2-Way F GT 150 Series (BK)

Connector Part Information

• | 15326806

• | 2-Way M GT 150 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | OG | 2740 | Battery Positive Voltage | A | OG | 2740 | Battery Positive Voltage
B | WH | 1310 | EVAP Canister Vent Solenoid Control | B | WH | 1310 | EVAP Canister Vent Solenoid Control

#### C408 Headliner to Body Harness-- Rear

Connector Part Information |

• | 15336888

• | 12-Way F GT 150/280 Series (BK)

Connector Part Information

• | 15336891

• | 12-Way M GT 150/280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | D-GN/WH | 368 | Right Audio Signal | A | D-GN/WH | 368 | Right Audio Signal
B | -- | 814 | Drain Wire | B | Bare | 814 | Drain Wire
C | BK/WH | 372 | Audio Common | C | BK/WH | 372 | Audio Common
D | BN/WH | 367 | Left Audio Signal | D | BN/WH | 367 | Left Audio Signal
E | D-BU | 601 | Data Clock Signal | E | D-BU | 601 | Data Clock Signal
F | BK | 650 | Ground | F | BK | 650 | Ground
G | OG | 1340 | Battery Positive Voltage | G | OG | 1340 | Battery Positive Voltage
H | PU | 1807 | Class 2 Serial Data | H | PU | 1807 | Class 2 Serial Data

#### C409 Rear Wheel Speed Sensors to Body Harness

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series (BK)

Connector Part Information

• | 12160825

• | 4-Way M Metri-Pack 150 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BK | 884 | Left Rear Wheel Speed Sensor | A | BK | 884 | Left Body to I/P Inline
B | BN | 882 | Right Rear Wheel Speed Sensor | B | BN | 882 | Left Body to I/P Inline
C | WH | 883 | Right Rear Wheel Speed Sensor | C | WH | 883 | Left Body to I/P Inline
D | RD | 885 | Left Rear Wheel Speed Sensor | D | RD | 885 | Left Body to I/P Inline

#### C493 Liftgate to Body Harness (Wagon)

Connector Part Information |

• | 12047886

• | 8-Way F Metri-Pack 150 Series (BK)

Connector Part Information

• | 12089526

• | 8-Way M Metri-Pack 150 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | WH | 393 | Rear Window Wiper Motor Control | A | WH | 393 | Rear Window Wiper Motor Control
B | YE | 143 | Accessory Voltage | B | YE | 143 | Accessory Voltage
C | BK | 650 | Ground | C | BK | 650 | Ground
D | GY | 382 | Trunk Release Enable Relay Switch Supply Voltage | D | GY | 382 | Trunk Release Enable Relay Switch Supply Voltage
E | RD/BK | 744 | Rear Compartment Lid Adjar Switch Signal | E | RD/BK | 744 | Rear Compartment Lid Adjar Switch Signal
F | L-BU | 20 | Stop Lamp Supply Voltage | F | L-BU | 20 | Stop Lamp Supply Voltage
G | BK | 305 | Trunk Key Switch Signal | G | BK | 305 | Trunk Key Switch Signal
H | OG | 340 | Battery Positive Voltage | H | OG | 340 | Battery Positive Voltage

#### C495 Liftgate/Defogger Harness to Body Harness (Wagon)

Connector Part Information |

• | 15318080

• | 2-Way F Metri-pack 280 Series (BK)

Connector Part Information

• | 15336392

• | 2-Way M Metri-Pack 280 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1 | BN | 9 | Park Lamp Supply Voltage | 1 | BN | 9 | Park Lamp Supply Voltage
2 | PU | 293 | Rear Defog Element Supply Voltage | 2 | PU | 293 | Rear Defog Element Supply Voltage

#### C498 Body Harness to Right Tail Lamp Harness (Sedan)

Connector Part Information |

• | 12064762

• | 6-Way F Metri-pack 150 Series (GY)

Connector Part Information

• | 12064763

• | 6-Way M Metri-Pack 150 Series (GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BN | 9 | Park Lamp Supply Voltage | A | BN | 9 | Park Lamp Supply Voltage
B | L-BU | 20 | Stop Lamp Supply Voltage | B | L-BU | 20 | Stop Lamp Supply Voltage
C | D-BU | 15 | Right Turn Signal Lamps Supply Voltage | C | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
D | BK | 650 | Ground | D | BK | 650 | Ground
E | L-GRN | 24 | Backup Lamp Supply Voltage | E | L-GRN | 24 | Backup Lamp Supply Voltage
F | -- | -- | Not Used | F | -- | -- | Not Used

#### C499 Body Harness to Left Tail Lamp Harness (Sedan)

Connector Part Information |

• | 12064762

• | 6-Way F Metri-pack 150 Series (GY)

Connector Part Information

• | 12064763

• | 6-Way M Metri-Pack 150 Series (GY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BN | 9 | Park Lamp Supply Voltage | A | BN | 9 | Park Lamp Supply Voltage
B | L-BU | 20 | Stop Lamp Supply Voltage | B | L-BU | 20 | Stop Lamp Supply Voltage
C | D-BU | 14 | Left Turn Signal Lamps Supply Voltage | C | D-BU | 14 | Left Turn Signal Lamps Supply Voltage
D | BK | 650 | Ground | D | BK | 650 | Ground
E | L-GRN | 24 | Backup Lamp Supply Voltage | E | L-GRN | 24 | Backup Lamp Supply Voltage
F | -- | -- | Not Used | F | -- | -- | Not Used

#### C505 Body Harness to Driver Door Harness

Connector Part Information |

• | 15326835

• | 8-Way F GT150 Series (BK)

Connector Part Information

• | 15326840

• | 8-Way M GT150 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | L-GN | 89 | Driver Mirror Motor Down Control | A | L-GN | 89 | Driver Mirror Motor Down Control
B | WH | 81 | Driver Mirror Motor Right Control | B | WH | 81 | Driver Mirror Motor Right Control
C | OG/BK | 781 | Driver Door Lock Switch Unlock Signal | C | RD/BK | 780 | Driver Door Lock Switch Unlock Signal
D | RD/BK | 780 | Driver Door Lock Switch Lock Signal | D | OG/BK | 781 | Driver Door Lock Switch Lock Signal
E | OG | 340 | Battery Positive Voltage | E | OG | 340 | Battery Positive Voltage
F | L-BU | 82 | Driver Mirror Motor Left Control | F | L-BU | 82 | Driver Mirror Motor Left Control
G | L-BU | 82 | Driver Mirror Motor Left Control | G | L-BU | 82 | Driver Mirror Motor Left Control
H | -- | -- | Not Used | H | -- | -- | Not Used

#### C507 Body Harness to Driver Door

Connector Part Information |

• | 15326829

• | 6-Way F GT 150 Series (BK)

Connector Part Information

• | 15326833

• | 6-Way M GT 150 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | GY | 118 | Left Front Speaker Output (-) | A | GY | 118 | Left Front Speaker Output (-)
B | TN | 201 | Left Front Speaker Output (+) | B | TN | 201 | Left Front Speaker Output (+)
C | BK | 550 | Ground | C | BK | 550 | Ground
D | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage | D | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage
E | BK | 550 | Ground | E | BK | 550 | Ground
F | YE | 743 | Accessory Voltage | F | YE | 743 | Accessory Voltage

#### C600 Body Harness to Front Passenger Door Harness

Connector Part Information |

• | 15326842

• | 10-Way F GT 150 Series (BK)

Connector Part Information

• | 15326847

• | 10-Way M GT 150 Series (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | D- GN | 117 | Right Front Speaker Output (-) | A | D- GN | 117 | Right Front Speaker Output (-)
B | L-GN | 200 | Right Front Speaker Output (+) | B | L-GN | 200 | Right Front Speaker Output (+)
C | BK | 450 | Ground | C | BK | 450 | Ground
D | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage | D | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage
E | L-GN | 89 | Mirror Motor Down Control | E | L-GN | 89 | Mirror Motor Down Control
F | WH | 81 | Driver Mirror Motor Right Control | F | WH | 81 | Driver Mirror Motor Right Control
G | RD/BK | 780 | Driver Door Lock Switch Lock Signal | G | RD/BK | 780 | Driver Door Lock Switch Lock Signal
H | OG/BK | 781 | Driver Door Lock Switch Unlock Signal | H | OG/BK | 781 | Driver Door Lock Switch Unlock Signal
J | OG | 340 | Battery Positive Voltage | J | OG | 340 | Battery Positive Voltage
K | L-BU | 82 | Driver Mirror Motor Left Control | K | L-BU | 82 | Driver Mirror Motor Left Control

#### C700 Body Harness to LR Door Harness

Connector Part Information |

• | 15318248

• | 15 Way F (BK)

Connector Part Information

• | 15305570

• | 15-Way M (BK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | GY | 295 | Door Lock Actuator Lock Control | 3 | GY | 295 | Door Lock Actuator Lock Control
4 | PU | 169 | Power Window Master Switch Left Rear Down Signal | 4 | PU | 169 | Power Window Master Switch Left Rear Down Signal
5 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal | 5 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal
6 | TN | 294 | Door Lock Actuator Unlock Control | 6 | TN | 294 | Door Lock Actuator Unlock Control
7-9 | -- | -- | Not Used | 7-9 | -- | -- | Not Used
10 | D-BU | 1307 | Power Window Master Switch Lockout Control | 10 | D-BU | 1307 | Power Window Master Switch Lockout Control
11 | L-BU/BK | 747 | Left Rear Door Ajar Switch Signal | 11 | L-BU/BK | 747 | Left Rear Door Ajar Switch Signal
12 | YE | 116 | Left Rear Speaker Output (-) | 12 | YE | 116 | Left Rear Speaker Output (-)
13 | WH | 199 | Left Rear Speaker Output (+) | 13 | WH | 199 | Left Rear Speaker Output (+)
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | OG | 1732 | Courtesy Lamps Supply Voltage | 15 | OG | 1732 | Courtesy Lamps Supply Voltage

#### C800 Inline Body to RR Door Harness

Connector Part Information |

• | 15318248

• | 15 Way F (BK)

Connector Part Information

• | 15305570

• | 15-Way M Black

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
1-2 | -- | -- | Not Used | 1-2 | -- | -- | Not Used
3 | GY | 295 | Door Lock Actuator Lock Control | 3 | GY | 295 | Door Lock Actuator Lock Control
4 | PU | 171 | Power Window Master Switch Right Rear Down Signal | 4 | PU | 171 | Power Window Master Switch Right Rear Down Signal
5 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal | 5 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal
6 | TN | 294 | Door Lock Actuator Unlock Control | 6 | TN | 294 | Door Lock Actuator Unlock Control
7-9 | -- | -- | Not Used | 7-9 | -- | -- | Not Used
10 | D-BU | 1307 | Power Window Master Switch Lockout Control | 10 | D-BU | 1307 | Power Window Master Switch Lockout Control
11 | L-GN/BK | 748 | Right Rear Door Ajar Switch Signal | 11 | L-GN/BK | 748 | Right Rear Door Ajar Switch Signal
12 | L-BU | 115 | Right Rear Speaker Output (-) | 12 | L-BU | 115 | Right Rear Speaker Output (-)
13 | D-BU | 46 | Right Rear Speaker Output (+) | 13 | D-BU | 46 | Right Rear Speaker Output (+)
14 | -- | -- | Not Used | 14 | -- | -- | Not Used
15 | OG | 1732 | Courtesy Lamps SuPUy Voltage | 15 | OG | 1732 | Courtesy Lamps SuPUy Voltage