For 1990-2009 cars

### Removal Procedure

1. Remove the rear transmission mount. Refer to Transmission Rear Mount Replacement in Automatic Transaxle 4T40-E/4T45-E.
2. Remove the rear transmission mount bracket to transmission bolts.
3. Remove the rear transmission mount bracket from the vehicle.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the transmission mount bracket to the transmission.

Tighten
Tighten the rear transmission mount bracket to transmission bolts to 90 N·m (66 lb ft).

2. Install the rear transmission mount. Refer to Transmission Rear Mount Replacement in Automatic Transaxle 4T40-E/4T45-E.