For 1990-2009 cars

### Removal Procedure

1. Disconnect the air pump solenoid harness connector.
2. Remove the vacuum hoses.
3. Remove the bolt.
4. Remove the air pump solenoid.

### Installation Procedure

1. Install the air pump solenoid.
2. Install and tighten the bolt.

Tighten
Tighten the air pump solenoid bolt to 10 N·m (89 lb in).

3. Install the vacuum hoses.
4. Connect the air pump solenoid harness connector. Push in the connector until a click is heard and pull back to confirm a positive engagement.