For 1990-2009 cars

### Removal Procedure

Important: Vehicles equipped with the L61 engine w/cruise control must have the left stabilizer removed with the vehicle in a raised position.

1. If equipped with a L61 engine w/cruise control, raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the stabilizer bar clamps.
3. Remove the bushings from the stabilizer shaft.

### Installation Procedure

1. Install the new stabilizer bushings with the opening facing forward.

Notice: Refer to Fastener Notice in the Preface section.

Important: Vehicles equipped with the L61 engine w/cruise control must have the left stabilizer installed with the vehicle in a raised position.

2. Install the stabilizer shaft clamps.

Tighten
Tighten the stabilizer clamp bolts to 20 N·m (15 lb ft).

3. If equipped with the L61 engine w/cruise control lower the vehicle.