For 1990-2009 cars

### Removal Procedure

Caution: Refer to SIR Caution in the Preface section.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Record all of the vehicle preset radio stations.
2. Turn OFF all the lamps and the accessories.
3. Make sure the ignition switch is in the OFF position.
4. Disconnect the battery negative cable from the battery.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: Clean any existing oxidation from the contact face of the battery terminal and battery cable using a wire brush before installing the battery cable to the battery terminal.

1. Connect the battery negative cable to the battery.

Tighten
Tighten the bolt to 17 N·m (13 lb ft).

2. Reset the radio stations and the clock.