For 1990-2009 cars

### Removal Procedure

1. Position the window half way down.
2. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement .
4. Remove the rear door trim plate.
5. Remove the foam insulator, from behind the trim plate.
6. Remove the lower rear window run channel. Refer to Rear Side Door Window Channel Replacement .
7. Remove the rear door window weatherstrip. Refer to Rear Side Door Window Weatherstrip Replacement .
8. Remove the window by tilting the rear of the window upward and sliding up and out.

### Installation Procedure

1. Install the window by tilting the rear of the window upward and sliding down and in.
2. Install the rear door window weatherstrip. Refer to Rear Side Door Window Weatherstrip Replacement .
3. Install the rear window run channel. Refer to Rear Side Door Window Channel Replacement .
4. Install the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement .
5. Install the rear door rim panel. Refer to Rear Side Door Trim Panel Replacement .
6. Install the foam insulator, behind the trim plate.
7. Install the rear door trim plate.
8. Operate the window to inspect the operation. If binding exists, inspect all of the weatherstrips and adjust as necessary.