For 1990-2009 cars

## Front Lower Control Arm Bushing Replacement Front

#### Tools Required

KM-508-A Control Arm Bushing Remover/Installer

### Removal Procedure

1. Remove the lower control arm. Refer to Lower Control Arm Replacement .
2. Using the KM-508-A , assemble the KM-508A-3 and KM-508-1 and press out the front control arm bushing.

### Installation Procedure

1. Using the KM-508-A , assemble the KM-508-1, KM-508-2 and KM-508-3 and press in the new front control arm bushing.
2. Install the lower control arm. Refer to Lower Control Arm Replacement .

## Front Lower Control Arm Bushing Replacement Rear

#### Tools Required

• | KM-671 Bushing Remover/Installer

• | KM-907 Control Arm Bushing Remover/Installer

### Removal Procedure

1. Remove the lower control arm. Refer to Lower Control Arm Replacement .
2. Using the KM-907 and theKM-671 , assemble the KM-907-21, KM-907-22 and the KM-671 and press out the rear control arm bushing.

### Installation Procedure

1. Using the KM-907 and theKM-671 , assemble the KM-907-23, KM-907-24 and the KM-671 and press in the rear control arm bushing.
2. Install the lower control arm. Refer to Lower Control Arm Replacement .