For 1990-2009 cars

### Tools Required

J 42059 Cigar Lighter Socket Remover

### Removal Procedure

1. Remove the power supply fuse.
2. Lift the cover.
3. Insert J 42059 into the socket sleeve. Tilt the tool into the slots on the sides of the socket sleeve.
4. Hold the plastic ring in place. Gently pull the socket out to remove the outlet.
5. Disconnect the electrical connector from the socket.

### Installation Procedure

1. Ensure that the plastic ring is in place.
2. Connect the electrical connector to the socket.
3. Install the socket into the opening until the socket clicks in place.