For 1990-2009 cars

### Removal Procedure

1. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement .
2. Disconnect the multifunction turn signal switch harness connector.
3. Remove the multifunction turn signal switch from the steering column.

### Installation Procedure

1. Install the multifunction turn signal switch to the steering column.
2. Connect the multifunction turn signal switch harness connector.
3. Install the steering column trim covers. Refer to Steering Column Trim Covers Replacement .