For 1990-2009 cars

## Drivetrain and Front Suspension Frame Insulator Replacement Outer

#### Tools Required

KM-907 Bushing Remover/Installer

### Removal Procedure

1. Remove the frame assembly. Refer to Frame Replacement .
2. Using the KM-907 , install the KM-907-11 KM-907-12, and the KM-907-30 in order to press out the outer damping bushing.

### Installation Procedure

1. Using the KM-907 , install the KM-907-13, KM-907-14 and the KM-907-30 in order to install the outer damping bushing.
2. Remove the frame assembly. Refer to Frame Replacement .

## Drivetrain and Front Suspension Frame Insulator Replacement Center

#### Tools Required

KM-907 Bushing Remover/Installer

### Removal Procedure

1. Remove the frame assembly (1). Refer to Frame Replacement .
2. Using the KM-907 , install the KM-907-11 KM-907-12 and the KM-907-30 in order to press out the center damping bushing.

### Installation Procedure

1. Using the KM-907 , install the KM-907-11, KM-907-22 and the KM-907-30 in order to install the center damping bushing.
2. Install the frame assembly (1). Refer to Frame Replacement .